**City of Baltimore**

**Department of Public Works**

**Code Reference for MV-RS HUL File**

The following fields are available:

Account Number

Meter Number

Comment – if a comment is entered by the meter reader

Read – the dial read, not including decimal places

Radio\_Read – includes decimal places for the raw read

Read Date

Read Time

Read Code:

C – Customer Read

F – Failed probe attempt

I – Fixed Network

N – Normal Read

O – Operator (meter reader) manual read or office read

S – Skipped Read

Blank – Missed Read

Skip Code

TCode 1 – Trouble Code 1

TCode 2 – Trouble Code 2

MReaderID – Meter Reader ID

PrevRead – the previous read for this meter dial

Read Method:

K – Keyed

N – No read

P – Probed optically

R – Radio

W – Wand

Text Prompt – text prompt provided to meter reader for type of read

RF\_ERT\_ID – ERT ID number

TamperStatus – tamper status of the meter